This is 550 Diaphragm Pump 12V Water Pump for Water Spray Fish Tank Reflux Pump. DC 12V 3.5L/Min Micro 550 Diaphragm Water Pump Watering Spray Aquarium Return Pump For Home Garden.

The configuration of the bath is according to the saving configuration: 12V2A power supply, bus connector, 4m 7 x 10 silicone tube, a 550 water pump, as for the shower nozzle, you can find a plastic bag, a good quality plastic bag or big cola bottle, The water intake and the amount of water can be equivalent.

Features :

1. Watering configuration: much the same, additional sprinklers and timers are required
2. 12V DC reflux diaphragm pump 550, the price is the price of a pump, without other accessories
3. Voltage: 12V, current: at least 2A, measured 1A is not able to bring
4. Suction: 3 meters or so, preferably 2 meters (no problem if the vertical height is 1.5 meters).
5. Head: 4-5 meters (head is not shot)
6. Highest temperature resistance 55°
7. Connect the mouth: the same as the outer diameter of the inlet and outlet, about 8.5mm, then connect the inner diameter of 7mm silicone tube tightly

|  |  |
| --- | --- |
| Cable Length (cm) | 28 |
| Weight (gm) | 480 |
| Shipment Weight | 0.5 kg |
| Shipment Dimensions | 9 × 6 × 5 cm |

